| Standards for Technology in Automotive Retail |
| Home - News Feed

Chapter 2. Common Components
Prev | STAR Level One | Next

## Chapter 2. Common Components

## 2.1. Overview

Regardless of whether a Generic Transport or a BOD Specific transport is being implemented, the overall message packaging will be the same. As was discussed earlier, the two transport mechanisms have to be inter operable at the messaging level. The following sections describe the message architecture that applies to both transport methods.

Prev | Up | Next
1.3. Web Service Interoperability Requirements | Home | 2.2. Message Packaging