| Standards for Technology in Automotive Retail |
| Home - News Feed

Appendix A. STAR Level One Check List
Prev |  | Next

## Appendix A. STAR Level One Check List

As specified by the STAR Transport Guidelines, each transport is to have a interoperability check list that is voluntarily filled out by the implementor. This check list should be sent back to STAR either via electronic format or via email submission. The check lists are a way for the STAR to guage the level of adoption as well as what portions of the specification are being implemented. This information is then used as input back to the Architecture Workgroup for further review and action on updates to the transport specification.

## A.1. Check List

This is the STAR Level 1 interoperability check list. Please fill this information out in a spreadsheet, and send back to info@starstandard.org. If the implementation has implemented the rule specified please mark with a Y. If the implementation has not implemented mark with a N. If the rule doesn't apply to your implementation please mark as NA.

Table A.1. STAR Level 1 Check List

Rule | Description | Implemented (Y, N, NA)
STAR1001 | All web services must be compliant to the rules and specifications outlined by the WS-I Basic Profile |
STAR1002 | Appropriate compliance markers are required as specified by the WS-I Conformance Claim Attachment Mechanisms document. |
STAR1003 | All implementations are required to support Username/Password for authentication |
STAR1004 | All implementations are REQUIRED to send information over HTTPS |
STAR1005 | All passwords are required to be sent as plain text |
STAR1008 | All services and clients must be compliant to the general Security requirements Outlined by the WS-I Basic Security Profile 1.0 .The optional attributes defined in the Profile is also to be relaxed in the STAR Implementation. |
STAR1009 | All STAR Web Services are REQUIRED to understand and handle the STAR Specific SOAP Faults. |
STAR1010 | All STAR soap fault error codes are REQUIRED to be be prefixed with STAR: and the appropriate STAR error code. i.e. STAR:Invalid Structure |
STAR1011 | All STAR soap fault error codes are REQUIRED to appear in the standard SOAP:Fault block. |
STAR1012 | SOAP Faults are for Critical Processing errors only. Informational or warning errors should not be sent as a SOAP Fault. |
STAR1013 | ConfirmBOD reason codes that are sent at the Warning or Informational status, SHOULD NOT trigger a resending of the BOD. |
STAR1014 | WS-Security errors must send the appropriate WS-Security SOAP Fault for the authorization being used. |
STAR1015 | STAR BOD Specific and Generic Transports must be message level interoperable. |
STAR1016 | Application level error messages MUST NOT be returned with a SOAP Fault, and MUST be returned using the appropriate BOD. |
STAR1017 | The service provider must keep track of contents that are deemed to have been received by the client to avoid resending. |
STAR1018 | A SOAP Header MUST contain one manifest element for each content element in the SOAP body. |
STAR1019 | A manifest is REQUIRED to have namespaceURI, element, contentID, and version attributes. Even though version is listed as optional it is REQUIRED for STAR BOD and DTS transports. |
STAR1020 | The client must be able to handle duplicate messages from a service provider. |

Prev |  | Next
STAR Interoperability Rules | Home | Normative References